## Welcome to the PoV-Ray Benchmark site

### Information

PoV-Ray is one of my favourite programs. That's why fast arithmetics is very important to me but the most benchmarks delivers only a global performance value. This small site could solve this problem by checking several systems for optimal PoV-Performance, not only PC's.
I need YOUR help for a complete overview about all CPU's and boards. Please send me your results and your description of the used machine. More stuff and more help are coming soon.

### Results

Please click here !

### Instructions

For your own results use the following scenes that are included in every official PoV-Ray distribution. Please do not turn on special features like antialiasing or so on. Take only the default parameters, e.g.
povray +v +w320 +h240 +b500 +i polywood.pov
Please have a look at the resolution of every scene:

Scene | Resolution
lemnisc2.pov | 320x240
skyvase.pov | 640x480
wg6.pov | 640x480
polywood.pov | 320x240

Send me your results using email to this address rs@informatik.tu-cottbus.de. Use a form like this:

    Machine
    -------------------------------------------------------------------------------------------
    CPU (e.g. Intel Pentium 133):
    Board (e.g. ASUS P54TP4):
    Cache (e.g. 256kB async):
    Memory (e.g. 32 MB EDO-RAM):
    System (e.g. DOS, Linux ):
    Version of PoV-Ray (e.g. official 3.0, own compilation of version 3.0 with gcc2.7.2):

    Results
    -------------------------------------------------------------------------------------------
    lemnisc2.pov (seconds):
    skyvase.pov (seconds):
    wg6.pov (seconds):
    polywood.pov (seconds):

    More information
    -------------------------------------------------------------------------------------------
    EMail:

### More stuff and links

The official Home of PoV-Ray
The incredible museum animation
Lot of PoV-Ray stuff and information
The official PoV-Benchmark page

Texture Magic | Texture Library | Pictures | WatchCat | Museum

28/04/97

Retour